common fault is boltwork coming loose so handle does not retract it fully. can usually be persuaded back into position without drilling.