Its another safe right next to it. Was a strange working mens club that had 3 safes in a row next to each other underfloor. Different commitee men had their own safes. The top bolt on this one had half snapped off and became jammed. The hydraulic arm had been broken for years apparently and quite often the safe was slamming shut. Ive removed the broken part and now it relies on just 2 locking points instead of 3. I explained that it may not pass insurance requirements but they weren`t interested in a new one.